{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":11,"n_cols":17,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Programm \"MZE\" berechnet MZB/t oder MZB in W/m²"]
[null,"nur sichtbarer Spektralbereich"]
[]
["Das Rechenblatt enthält eine benutzerdefinierte Funktion namens",null,null,null,null,"Um Makros/Funktionen zu aktivieren, klicken Sie auf \"Entwicklertools\" und dort auf \"Makrosicherheit\""]
["MZBe(Wellelange; Impulsdauer) und kann in jeder Zelle aufgerufen werden.",null,null,null,null,"Einstellungen für Makros: Alle Makros aktivieren"]
["Es werden mehrere Beispiele angegeben:",null,null,null,null,"Entwicklermakroeinstellungen: Zugriff … vertrauen"]
[]
[]
["Wellenlänge in nm:","Wl/nm",532,532,532,532,532,532,532,532,532,425,490,532,490,650,"nm"]
["Impulsdauer in s:","Ida/s",4.9999999999999997E-12,5.0000000000000003E-10,9.9999999999999995E-7,1.9000000000000001E-5,1,9,12,12,12,98,98,98,110,110,"s"]
["MZB/t wenn in J/m²","MZE/(W/m²)",{"$f":"MZBe(Wl,Ida)","v":30000000},{"$f":"MZBe(D9,D10)","v":5709804.8225790458},{"$f":"MZBe(E9,E10)","v":5000},272.63656719901314,18,10.392304845413264,10,10,10,1.0204081632653061,6.438340249797891,10,6.3095734448019334,10,"W/m²"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}